Considering the MIPS64 architecture presented in the following:

|  |  |  |
| --- | --- | --- |
| * + Integer ALU: 1 clock cycle   + Data memory: 1 clock cycle   + FP multiplier unit: pipelined 8 stages | * + FP arithmetic unit: pipelined 2 stages   + FP divider unit: not pipelined unit that requires 12 clock cycles   + branch delay slot: 1 clock cycle, and the branch delay slot disabled | * + forwarding enabled   + it is possible to complete instruction EXE stage in an out-of-order fashion. |

* Using the following code fragment, show the timing of the presented loop-based program and compute how many cycles does this program take to execute?

for (i = 0; i < 10; i++) {

result+=values[i]

}

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| .data |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | Clock  cycles |
| values: .word 1,2,3,4,5,6,7,8,9,10 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| result: .space 8 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **.text** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| MAIN: daddui R1, R0, 10 | F | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 5 |
| dadd R2, R0, R0 |  | F | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 1 |
| dadd R3, R0, R0 |  |  | F | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 1 |
| LOOP: ld R4, values(R2) |  |  |  | F | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 1 |
| dadd R3, R3, R4 |  |  |  |  | F | D | s | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 2 |
| daddi R2, R2, 8 |  |  |  |  |  | F | s | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 1 |
| daddi R1, R1, -1 |  |  |  |  |  |  |  | F | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 1 |
| bnez R1, LOOP |  |  |  |  |  |  |  |  | F | s | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 2 |
| sd R3, result(R0) |  |  |  |  |  |  |  |  |  |  | F | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 1 |
| halt |  |  |  |  |  |  |  |  |  |  |  | F | D | E | M | W |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 1 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 7+8\*10+1=88 | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | 88 |